|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  | | | |  |  |
|  | | **OUH Networks Contact** | | **Customer Engineer** |  | | | | |
| Name: | | Toby Rosoman | |  |  | | | | |
| Telephone: | | 01865 743223/07919 690888 | |  |  | | | | |
| Email: | | *Toby.Rosoman@ouh.nhs.uk* | |  |  | | | | |
|  |  |  |  |  | | | |  |  |
| **Firewall Information** | |  |  |  | | | |  |  |
|  | | **OUH Network VPN Peer** | | **Customer VPN Peer** |  | | | | |
| IP Address(s): | | 10.134.250.98 | |  |  | | | | |
| VPN/Firewall manufacturer, model and software version: | | *Cisco 5525-X, Ver 9.12..4(24)* | |  |  | | | | |
| Location: | | Oxford | |  |  | | | | |
| **IKEv2 Policy** | |  |  |  | |
|  | | | **OUH Network Default Crypto Settings** | |  | |
| IKE Version: | | | **IKEv2** | |  | |
| Encryption Scheme: | | | **AES-CBC-256** | |  | |
| PRF: | | | **HMAC-SHA256** | |  | |
| Diffie Hellman Group: | | | **Group 21** | |  | |
| IKE lifetime: | | | **82800 seconds** (23 hours) | |  | |
| Authentication: | | | **Pre-Shared Key – Supplied at the time of build** | |  | |
|  |  |  |  |  | | | |  |  |
| **IPSec proposal** | |  |  |  | | | |  |  |
|  | | | **OUH Network Default Crypto Settings** | |  | |
| IPsec protocol: | | | **IPSec** | |  | |
| Encryption Scheme: | | | **AES-CBC-256** | |  | |
| Integrity Hash: | | | **SHA256** | |  | |
| IPsec SA lifetime: | | | **28800 seconds** (8 hours) | |  | |
| PFS (perfect forward secrecy / DH Group): | | | **Group 21** | |  | |
| Note: Should your VPN hardware not support the above listed ciphers please amend. | | | | | | | | | |
| **Encryption Domain** | | | | |  | | | | |
| **OUH Dart Hosted Networks** | | | **Customer Networks** | |  | | | | |
| DART OUH PACs  IP: 10.134.128.213  AET: HDART1  Port: 10505 | | |  | |  | | | | |