|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |
|  | **OUH Networks Contact** | **Customer Engineer** |  |
| Name: | Toby Rosoman |  |  |
| Telephone: | 01865 743223/07919 690888 |  |  |
| Email: | *Toby.Rosoman@ouh.nhs.uk* |  |  |
|  |  |  |  |  |  |  |
| **Firewall Information** |  |  |  |  |  |
|   | **OUH Network VPN Peer** | **Customer VPN Peer** |  |
| IP Address(s): | 10.134.250.98 |  |  |
| VPN/Firewall manufacturer, model and software version: | *Cisco 5525-X, Ver 9.12..4(24)* |  |  |
| Location: | Oxford |  |  |
| **IKEv2 Policy** |  |  |  |
|  | **OUH Network Default Crypto Settings** |  |
| IKE Version: | **IKEv2** |  |
| Encryption Scheme: | **AES-CBC-256** |  |
| PRF: | **HMAC-SHA256** |  |
| Diffie Hellman Group: | **Group 21** |  |
| IKE lifetime: | **82800 seconds** (23 hours) |  |
| Authentication: | **Pre-Shared Key – Supplied at the time of build** |  |
|  |  |  |  |  |  |  |
| **IPSec proposal** |  |  |  |  |  |
|  | **OUH Network Default Crypto Settings** |  |
| IPsec protocol: | **IPSec** |  |
| Encryption Scheme: | **AES-CBC-256** |  |
| Integrity Hash: | **SHA256** |  |
| IPsec SA lifetime: | **28800 seconds** (8 hours) |  |
| PFS (perfect forward secrecy / DH Group): | **Group 21** |  |
| Note: Should your VPN hardware not support the above listed ciphers please amend. |
| **Encryption Domain** |  |
| **OUH Dart Hosted Networks** | **Customer Networks** |  |
| DART OUH PACsIP: 10.134.128.213AET: HDART1Port: 10505 |  |  |